{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":59,"n_cols":5,"rows_kept":59,"merged":[[0,0,0,4]],"flags":["formulas_cached_only"]}
["招标工程量清单"]
["序号","项目名称","项目特征描述","计量\r\n单位","工程量"]
[null,"土建部分"]
["1","新建实心隔墙","1.砖品种、规格、强度等级:MU15页岩砖、240mm×115mm×53mm\r\n2.墙体类型:隔墙\r\n3.墙体厚度:200mm\r\n4.砂浆强度等级:M5水泥砂浆","m3","5.44"]
["2","新建砌块隔墙","1.砖品种、规格、强度等级:加气混凝土砌块\r\n2.墙体类型:隔墙\r\n3.墙体厚度:150mm\r\n4.砂浆强度等级:M5混合砂浆","m3","45"]
["3","构造柱 C25","1.混凝土种类 ：现浇混凝土\r\n2.混凝土强度等级;C25","m3","4.99"]
["4","构造柱-模板","1.构件类型：构造柱-模板\r\n2.本项目投标人应根据设计图纸,施工组织设计,现场实际情况和企业自身情况综合报价,不论采用何种支模方式及材质均执行该综合单价\r\n3.支模要求满足设计及施工验收规范","m2","99.84"]
["5","过梁 C25","1.混凝土种类 ：现浇混凝土\r\n2.混凝土强度等级;C25","m3","0.5"]
["6","过梁-模板","1.构件类型：过梁-模板\r\n2.本项目投标人应根据设计图纸,施工组织设计,现场实际情况和企业自身情况综合报价,不论采用何种支模方式及材质均执行该综合单价\r\n3.支模要求满足设计及施工验收规范","m2","6.5"]
["7","圈梁 C25","1.混凝土种类 ：现浇混凝土\r\n2.混凝土强度等级;C25","m3","2.4"]
["8","圈梁-模板","1.构件类型：圈梁-模板\r\n2.本项目投标人应根据设计图纸,施工组织设计,现场实际情况和企业自身情况综合报价,不论采用何种支模方式及材质均执行该综合单价\r\n3.支模要求满足设计及施工验收规范","m2","32.01"]
["9","现浇构件钢筋 HRB400 Φ10以内","1.钢筋种类、规格：HRB400级钢筋，规格φ6-10","t","0.292"]
["10","现浇构件钢筋 HRB400 Φ12-14","1.钢筋种类、规格：HRB400级钢筋，规格φ12-14","t","0.876"]
["11","成品塑钢隔断(H=1800)","1.隔断材料品种、规格、颜色 ：成品塑钢隔断(门900*1200)","m2","10.44"]
["12","炉渣回填","1.垫层材料种类、配合比、厚度：炉渣回填","m3","15.54"]
["13","800*800地砖楼地面","1.找平层材料种类、厚度：1:3水泥砂浆20mm厚 \r\n2.结合层厚度、砂浆配合比：20mm厚1:2干硬性水泥砂浆 \r\n3.面层材料品种、规格：普通地砖 800×800 \r\n4.嵌缝材料种类：白水泥浆","m2","396.65"]
["14","400*400地砖楼地面","1.找平层材料种类、厚度：1:3水泥砂浆20mm厚 \r\n2.结合层厚度、砂浆配合比：20mm厚1:2干硬性水泥砂浆 \r\n3.面层材料品种、规格：防滑地砖400*400\r\n4.嵌缝材料种类：白水泥浆","m2","16.75"]
["15","1.5厚JS-Ⅱ聚合物水泥防水-地面","1.卷材品种、规格、厚度：1.5厚JS-Ⅱ聚合物水泥防水\r\n2.防水层数：一层\r\n3.反边高度：至吊顶","m2","16.75"]
["16","1.5厚JS-Ⅱ聚合物水泥防水-墙面","1.防水膜品种 ：1.5厚JS-Ⅱ聚合物水泥防水涂料一道","m2","76.98"]
["17","400*800瓷砖内墙面","1 .400*800面砖\r\n2 .专用陶瓷胶粘剂\r\n3 .8厚1:3水泥砂浆(搓毛)\r\n4 .12厚1:3水泥砂浆打底\r\n5 .1.5mm厚JS-Ⅱ型水泥聚合物防水涂料两道(四周墙面上翻至吊顶）（另计）\r\n6 .基层处理","m2","76.98"]
["18","吊顶天棚","1.吊顶形式：不上人型U型轻钢龙骨吊顶，平面\r\n2.龙骨材料种类、规格、中距：φ6.5钢筋吊杆、双向吊点、中距900mm。U型轻钢主龙骨38mm×12mm×1.0mm，中距1000mm；次龙骨50mm×19mm×0.5mm，中距450mm；覆面横撑龙骨50mm×19mm×0.5mm，中距600mm\r\n3.基层材料种类、规格：纸面石膏板基层，2400mm×1200mm×9.5mm防潮型普通板，用镀锌螺丝与覆面龙骨固定\r\n4.面层材料品种、规格、品牌、颜色：刷白色乳胶漆底漆一遍、面漆两遍（另计）\r\n5.嵌缝材料种类：纸面石膏板接缝处刮嵌缝腻子，贴嵌缝纸带","m2","16.75"]
["19","乳胶漆天棚","1.基层类型：墙面一般抹灰面\r\n2.油漆品种、刷漆遍数：乳胶漆底漆一遍，面漆两遍","m2","413.4"]
["20","成品实木踢脚板","1.踢脚线高度 ：80\r\n2.成品实木踢脚板","m2","17.04"]
["21","墙面一般抹灰","1.墙体类型：砖内墙\r\n2.底层厚度、砂浆配合比：基层上刷素水泥浆一遍、9mm厚1:1:6混合砂浆打底、再抹7mm厚1:1:6混合砂浆\r\n3.面层厚度、砂浆配合比：5mm厚1:0.3:2.5混合砂浆罩面压光\r\n4.装饰面材料种类：满刮腻子胶二遍、刷乳胶漆（另计）","m2","790.2"]
["22","乳胶漆内墙面","1.基层类型：墙面一般抹灰面\r\n2.腻子种类：石膏粉腻子\r\n3.刮腻子要求：清理基层，修补，砂纸打磨；满刮腻子一遍，找补两遍\r\n4.油漆品种、刷漆遍数：乳胶漆底漆一遍，面漆两遍","m2","816.6"]
["23","断桥铝合金窗","1.窗代号及洞口尺寸 ：综合\r\n2.框、扇材质 ：铝合金\r\n3.玻璃品种、厚度;中空玻璃5+20+5","m2","132"]
["24","全玻自由门","1.门类型：全玻自由门\r\n2.框外围尺寸：:2000mmX3000mm\r\n3.玻璃品种、厚度：12mm厚钢化玻璃\r\n4.五金材料：不锈钢管子拉手、不锈钢夹具","m2","32"]
["25","木质门带套","1.门代号及洞口尺寸 ：木质门带","m2","11.34"]
["26","钛合金门","1.门代号及洞口尺寸 ：钛合金门\r\n2.门框或扇外围尺寸 ：综合\r\n3.门框、扇材质 ：钛合金门\r\n4.玻璃品种、厚度：5mm厚平玻\r\n5.五金材料：闭门器、管子拉手、门碰珠、门锁(型号详设计)","m2","3.2"]
["27","石膏板双面隔墙","1.墙体类型：砖基层\r\n2.龙骨材料种类、规格、中距：40mm×40mm一等杉木龙骨，中距300mm×300mm\r\n3.基层材料种类、规格：木工板10mm厚\r\n4.面层材料品种、规格、品牌、颜色：纸面石膏板 12mm厚\r\n5.压条材料种类、规格：15mm宽硬木压条（图案及部位见设计图）\r\n6.面层材料品种、规格、品牌、颜色：天棚面满刮腻子两遍，刷白色乳胶漆底漆一遍、面漆两遍\r\n7.嵌缝材料种类：纸面石膏板接缝处刮嵌缝腻子，贴嵌缝纸带","m2","31"]
["28","洗漱台面","1.材料品种、规格、品牌、颜色：大理石板 厚20mm\r\n2.支架、配件品种、规格、品牌：40mm×3mm角钢托架\r\n3.油漆品种、刷漆遍数：角钢托架刷红丹防锈漆一遍、灰铅油二遍","m2","1.06"]
["29","橱柜","1.橱柜、吊柜","m","4"]
["30","吊柜"," ","m","4"]
["31","隔断柜","1.隔断柜","m2","3.6"]
["32","石材台面前台柜","1.石材台面前台柜","m","4"]
["33","形象墙1.5万","1.形象墙1.5万","项","1"]
[" ","分部小计 ",null," "," "]
[" ","安装部分 ",null," "," "]
["34","配电箱 AL","1.名称：配电箱 AL\r\n2.规格、型号：根据系统图加工制作，带门锁\r\n3.安装形式：详设计\r\n4.其他：箱体安装、含箱内电器元件、盘柜配线、开孔、压焊接线端子、接地、盘柜防火堵洞\r\n5.满足设计及规范要求","台","1"]
["35","吸顶节能灯","1.名称：吸顶节能灯\r\n2.型号、规格：1200*200\r\n3.安装形式：吸顶安装\r\n4.其他：满足设计及规范要求","套","42"]
["36","筒灯","1.名称：筒灯\r\n2.型号、规格：详设计\r\n3.安装形式：吸顶安装\r\n4.其他：满足设计及规范要求","套","12"]
["37","电气配管 PC20","1.名称：阻燃半硬塑料管敷设\r\n2.材质、规格：PC20\r\n3.配置形式及部位：砖、混凝土结构暗配\r\n4.本项目含预留或开凿管槽及修补，管内穿铁丝\r\n5.其他:满足设计及规范要求","m","647.88"]
["38","电气配线 BV-6mm2","1.配线形式：暗配\r\n2.导线型号、材质、规格：BV-6mm2\r\n3.敷设部位或线制：综合考虑\r\n4.其它：本项目双色线价差、预留量考虑在综合单价内","m","746.4"]
["39","电气配线 BV-2.5mm2","1.配线形式：暗配\r\n2.导线型号、材质、规格：BV-2.5mm2\r\n3.敷设部位或线制：综合考虑\r\n4.其它：本项目双色线价差、预留量考虑在综合单价内","m","611.4"]
["40","电气配线 BV-4mm2","1.配线形式：暗配\r\n2.导线型号、材质、规格：BV-4mm2\r\n3.敷设部位或线制：综合考虑\r\n4.其它：本项目双色线价差、预留量考虑在综合单价内","m","772.44"]
["41","安全型单相二、三极暗装插座","1.名称：安全型单相二、三极暗装插座\r\n2.型号、规格：16A 250V\r\n3.安装方式：墙上暗装，综合考虑","个","45"]
["42","网络插座","1.名称：网络插座\r\n2.安装方式：综合考虑\r\n3.底盒材质、规格：详设计\r\n4.其他：满足设计及规范要求","个","23"]
["43","空调插座","1.名称：空调插座 \r\n2.型号、规格：16A 250V\r\n3.安装方式：墙上暗装，综合考虑","个","2"]
["44","翘板式单联暗开关","1.名称：翘板式单联暗开关\r\n2.型号、规格：250V  10A\r\n3.安装方式：底距地1.2m安装","个","10"]
["45","翘板式双联暗开关","1.名称：翘板式双联暗开关\r\n2.型号、规格：250V  10A\r\n3.安装方式：底距地1.2m安装","个","2"]
["46","翘板式三联暗开关","1.名称：翘板式三联暗开关\r\n2.型号、规格：250V  10A\r\n3.安装方式：底距地1.2m安装","个","2"]
["47","开关插座灯具接线盒","1.名称：开关插座灯具接线盒\r\n2.材质：塑料\r\n3.配置形式及部位：砖混凝土结构暗配","个","138"]
["48","洗脸盆","1.材质：陶瓷 \r\n2.规格、类型：详设计 \r\n3.组装形式：详设计 \r\n4.附件名称、数量：带水嘴、恒温混合阀 DN15等所有配件","组","2"]
["49","瓷蹲式大便器","1.材质：陶瓷 \r\n2.规格、类型：带水箱 \r\n3.组装形式：详设计 \r\n4.附件名称、数量：含角阀、软管等附件","组","4"]
["50","小便器","1.材质：陶瓷 \r\n2.规格、类型：详设计\r\n3.组装形式：详设计 \r\n4.附件名称、数量：含角阀、软管等附件","组","1"]
["51","成品拖布池","1.材质：陶瓷","组","2"]
["52","地漏 DN50","1.名称：地漏\r\n2.型号、规格：DN50\r\n3.其它：本项目含存水弯供应与安装","个","3"]
["53","天花机空调","1.天花机空调\n2.规格型号：KFR-72GW/BPR3YC(B3)，额定制冷量7.2（1.8~8.9），制热量9.2（1.8~10），面板尺寸;950*950*55,室外机尺寸：950*300*750\n3.机型：三匹变频冷暖","台","5"]
["54","挂机空调","1.挂机\r\n2.规格型号：35-AQD600(B3)","台","2"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}